
* No more than 4 Heater Strips per Transformer
* Do not install product where you expect standing water
* Do not directly connect into 120 VAC
* Do not penetrate or puncture material with metal objects
* Do not exceed minimum (3 Ft) and maximum (12-14 Ft) material lengths
* Do not exceed 30ft-wiring limitation on Secondary Circuit
* Do not place transformer within 4 inches of combustible materials
* Always use 10 AWG between Transformer and Heater Strip

✗

**Do not** use Linesman, needlenose or any other type of pliers to secure Splice Connector onto material!

✓

For proper crimping please use a flat nose-crimping tool!

✗✓